**SECTION 08 5667**

**BULLET-RESISTANT STEEL TRANSACTION WINDOWS**

This section includes editing notes to assist the user in editing the section to suit project requirements. These notes are included as hidden text, and can be revealed or hidden by one of the following methods:

Microsoft Word 2013: Display the FILE tab on the ribbon, click OPTIONS, then DISPLAY. Select of deselect HIDDEN TEXT.

Microsoft Word 2010: Display the FILE tab on the ribbon, click OPTIONS, then on left menu click on DISPLAY. Under ALWAYS SHOW THESE select or deselect HIDDEN TEXT.

Corel WordPerfect: From the pull-down menus select VIEW, then select or deselect the HIDDEN TEXT option.

This master specification section has been prepared by ARMORTEX for use in the preparation of a project specification section covering bullet-resistant steel transaction window assemblies, fixed or horizontally sliding, and baffle type windows. ARMORTEX steel transaction window assemblies are available in Ballistic Levels 1 through 8, except that horizontally sliding widows are available in Levels 1 through 4 only.

The following should be noted in using this specification:

Hypertext links to specific websites are included after manufacturer names and names of organizations whose standards are referenced within the text, to assist in product selection and further research. Hypertext links are contained in parenthesis and shown in blue, e.g.:

 ([www.spexplus.net](http://www.spexplus.net))

Optional text requiring a selection by the user is enclosed within brackets, e.g.: "Section [09 0000.] [\_\_\_\_\_.]"

Items requiring user input are enclosed within brackets, e.g.: "Section [\_\_\_\_\_ - \_\_\_\_\_\_\_\_]."

Optional paragraphs are separated by an "OR" statement, e.g.:

\*\*\*\* OR \*\*\*\*

Sustainable requirements are included for projects requiring LEED certification, and are included as green text. For additional information on LEED, visit the U.S. Green Building Council website at [www.usgbc.org](http://www.usgbc.org).

For assistance on the use of the products in this section, contact ARMORTEX by calling 800-880-8306, by email at info@armortex.com, or visit their website at [www.armortex.com](http://www.armortex.com).

1. **GENERAL**
	1. SUMMARY

Edit the following paragraphs to include only those items specified in this section.

* + 1. Section Includes:
			1. Bullet-resistant [fixed] [horizontally sliding] steel transaction window assemblies.

Coordinate the following paragraphs with other sections in the project manual.

* + 1. Related Sections:
			1. Division 01: Administrative, procedural, and temporary work requirements.
	1. REFERENCES
		1. American Welding Society (AWS) ([www.aws.org](http://www.aws.org)) D1.3/D1.3M - Structural Welding Code - Sheet Steel.
		2. ASTM International (ASTM) ([www.astm.org](http://www.astm.org)) A1008/A1008M - Standard Specification for Steel, Sheet, Cold-Rolled, Carbon, Structural, High-Strength Low-Alloy and High-Strength Low-Alloy with Improved Formability.
		3. Underwriters Laboratories (UL) [(www.ul.com](http://www.ul.com)) 752 - Bullet Resisting Equipment.
	2. SYSTEM DESCRIPTION
		1. Design Requirements:
			1. Provide window frames of “non-ricochet type" intended to permit capture and retention of attacking projectile, lessening potential of random injury or lateral penetration.
			2. Two way "natural voice" communication permitted by design of vertical side frames and glazing technique.
	3. SUBMITTALS

Limiting submittals to only those actually required helps to minimize liability arising from the review of submittals. Minimize submittals on smaller, less complex projects.

Include the following for submission of shop drawings, product data, and samples for the Architect's review.

* + 1. Submittals for Review:
			1. Shop Drawings: Include window profiles and sizes, type and spacing of frame anchors, reinforcement size and locations, details of joints and connections, and welding details.
			2. Product Data: Include product description for window assemblies including bullet-resistant ratings.

Include the following is a powder coated finish is desired. Edit to suit project requirements.

* + - 1. Samples: [2 x 2] [\_\_ x \_\_] inch coating samples [showing available colors.] [in specified color.]

Include the following for submission of sustainable design submittals.

* + 1. Sustainable Design Submittals:
			1. Recycled Content: Certify percentages of post-consumer and pre-consumer recycled content.
			2. Regional Materials: Indicate cost of products harvested, extracted, recovered, or manufactured within 500 mile radius of Project site.

Include the following for submission of closeout submittals on cleaning of glazing materials.

* + 1. Closeout Submittals:
			1. Maintenance Data: Include instructions for cleaning of glazed panels.
	1. QUALITY ASSURANCE

Edit the following to suit project requirements; delete if this information is indicated on Drawings. Horizontally sliding windows are available in Levels 1 through 4 only.

* + 1. Transaction Window Assemblies: Ballistic Level [1,] [2,] [3,] [4,] [5,] [6,] [7,] [8,] tested to UL 752.
	1. DELIVERY, STORAGE AND HANDLING
		1. Store window assemblies upright in protected, dry area, off ground or floor, with at least 1/4 inch space between individual units.
		2. Do not cover with non vented coverings that create excessive humidity.
		3. Remove wet coverings immediately.
1. **PRODUCTS**
	1. MANUFACTURERS
		1. Contract Documents are based on products by ARMORTEX, 5926 Corridor Parkway, Schertz, Texas, 800-880-8306, [www.armortex.com](http://www.armortex.com).

Edit the following to indicate whether or not substitutions will be permitted for the products in this section.

* + 1. Substitutions: [Under provisions of Division 01.] [Not permitted.]
	1. MATERIALS
		1. Steel Sheet:
			1. ASTM A1008/1008M, cold rolled, free from scale, pitting, coil breaks, and other surface defects.

Insert percent of recycled content for steel in the following paragraph; contact ARMORTEX to verify current recycled content availability.

* + - 1. Recycled content: Minimum [\_\_] percent, with minimum [\_\_] percent classified as post consumer.

Include the following for Ballistic Level 1 through 3 windows.

* + 1. Bullet-Resistant Composite: UL Listed Bullet Resistant Composite by ARMORTEX, of UL Ballistic Level equal to specified frame ballistic protection level.

Include the following for Ballistic Level 4 through 8 windows.

* + 1. Ballistic Steel: Hi-Hard Ballistic Steel, of UL Ballistic Level equal to specified frame ballistic protection level.
		2. Glazing:
			1. UL Listed [laminated glass.] [glass/polycarbonate composite.] [Glass-clad polycarbonate.] [Multi-ply polycarbonate.] [Acrylic polycarbonate composite.] [\_\_\_\_\_.]
			2. Bottom edge of glazing panel provided with 18 gage stainless steel cap.

Include the following for horizontally sliding windows (Ballistic Levels 1 through 4 only).

* + 1. Track and Hangers:
			1. Stainless steel 12 gage track guard and guide.
			2. Aluminum 1500 series sliding roller track and wheeled hangers.
	1. FABRICATION
		1. Frames:

Edit the following to suit project requirements. Windows requiring Ballistic Level 1 through 3 use bullet-resistant composite cores; Ballistic Level 4 though 8 require ballistic steel cores.

* + - 1. Fabricate from 16 gage steel lined with [bullet-resistant composite.] [ballistic steel.]
			2. Bullet-resistant rating equivalent to or greater than glazing.
			3. Weld frame corners; knock-down and mechanical joints not acceptable.
			4. Frame modules capable of being joined with other frame modules to form continuous line.
			5. Replacement of glazing from secure side of window, not requiring removal of frame from opening.
		1. Shelf: Minimum 2 inches thick with recessed dip tray, full width of window x minimum 12 inches deep, centered under glazing, covered with [[black] [\_\_\_\_] high pressure laminate.] [18 gage stainless steel.]
		2. Dip Tray: Model RMDT1016, 16 gage stainless steel, 10 x 16 inches to outside edge of flanges, clear 1-5/8 inch open depth under glazing.
		3. Welding: In accordance with AWS D1.3/D1.3M. Grind exposed welds flush and smooth.
		4. Finish work neat and free from defects.
		5. Allowable Tolerances: Plus or minus 1/16 inch for frame opening width, height, diagonal dimensions, and overall width and height (outside to outside).
	1. FINISHES

Include the following for a standard prime painted finish.

* + 1. Steel:
			1. Dress tool marks and surface imperfections to smooth surfaces.
			2. Clean and chemically treat steel surfaces.
			3. Apply manufacturer's standard rust inhibiting gray primer paint.

\*\*\*\* OR \*\*\*\*

Include the following for an optional powder coated finish.

* + - 1. Apply manufacturer’s standard polyester powder coat, sprayed and baked, [\_\_\_\_] [custom] color [to be selected from manufacturer’s full color range].
		1. Stainless Steel: No. 3 brushed finish.
1. **EXECUTION**
	1. INSTALLATION
		1. Install window assemblies in accordance with manufacturer’s instructions and approved Shop Drawings.
		2. Set plumb and level.
		3. Secure to adjacent construction using fastener type best suited to application.
		4. Field alterations to window assemblies not permitted unless approved in advance by manufacturer and Architect.
	2. ADJUSTING

Edit the following to suit project requirements.

* + 1. Touch up minor scratches and abrasions in [primer paint] [finish coat] to match factory finish.

END OF SECTION